The corrosion rate (mm/year) can be calculated as

where *K* is a constant equal to 8.76x104, is the mass loss in grams, *a* is the area in cm2, *T* is the time of corrosion exposure in hours and *D* is the density of steel i.e.,7.8g/cm3.